VERSION 23.9.0.b16-3-gd95f4a0e
'FCC MAIN QUAD (34 x 0.7 mm 78/91) 361 T/m, 120 um (2.5 /1.5%)                      '
''
'/home/mkarppin/FCC/MQ/FCC_mk.cadata                                                '
''

&OPTION
  LEND=T         LWEDG=F        LPERS=F        LQUENCH=F      LALGO=F        LQUENCH0D=F    
  LMIRIRON=F     LBEMFEM=F      LPSI=F         LSOLV=F        LIRON=F        LMORPH=F       
  LHMO=F         LHARD=F        LPOSTP=F       LPEAK=F        LINMARG=F      LMARG=F        
  LSELF=F        LMQE=F         LINDU=F        LEDDY=F        LSOLE=F        LFLUX=F        
  LFIELD3=F      LSELF3=F       LBRICK=F       LLEAD=F        LVRML=F        LOPERA=F       
  LOPER20=F      LANSYS=F       LRX2ANS=F      LANS2RX=F      LDXF=F         LMAP2D=F       
  LMAP3D=T       LEXPR=F        LFIL3D=F       LFIL2D=F       LCNC=F         LANSYSCN=F     
  LWEIRON=F      LCATIA=F       LEXEL=F        LQVOLT=F       LFORCE2D=F     LQUNPLOT=F     
  LGRAPHCSV=F    LAXIS=T        LIMAGX=T       LIMAGY=T       LRAEND=F       LMARKER=F      
  LROLER2=F      LROLERP=T      LIMAGZZ=F      LSUPP=T        LSTEP=F        LSKIPDPL=T     
  LIFF=F         LICCA=F        LICC=F         LICCIND=F      LITERNL=F      LTOPO=F        
  LQUEN3=F       LAYER=T        LEULER=T       LHEAD=T        LPLOT=T        LVERS52=T      
  LHARM=F        LMATRF=F       LF3LIN=F       LKVAL=F        LSKIPTPL=T     
  /

GLOBAL2DOPTION 0

GLOBAL3D 0

BLOCK 4
  1     1    6    25.0  0.8698      0    16126 FCMQ3491Q   2  17     0     0    25   1
  2     1    3    25.0 23.0757     28    16126 FCMQ3491Q   2  17     0     0    25   2
  3     1    9    38.6  0.3972      0    16126 FCMQ3491Q   2  17     0     0    25   3
  4     1    4    38.6 21.3345     25    16126 FCMQ3491Q   2  17     0     0    25   4
 no  type  nco  radius     phi  alpha  current  condname  n1  n2  imag  turn  disc  ne

BLOCKOPTION 1
  1  CONTR  0.003     0 /
 no string  value block

BLOCK3D 4
  1    31 86.2825 1.9172 81.134 0.05   0  12.5  3.1780
  2    31 89.2228 1.6384 60.000 0.05   0  12.5  3.0278
  3    31 78.6012 1.8255 74.344 0.05   0  12.5  3.0837
  4    31 87.5830 1.8173 58.150 0.05   0  12.5  3.3364
 ne  type    beta     bo     zo   wi  wo  hwed  horder

BLOCKOPTION3D 4
  1 NSTRDIS      5     1 /
  2 NSTRDIS      5     2 /
  3 NSTRDIS      5     3 /
  4 NSTRDIS      5     4 /
 no  string  value block

LEAD 0

BRICK 0

IRONYOKEOPTIONS /
      0
  scale

             75.255            100
         inrad       reperm

      1
  symtype

      2     2     3
  yzplane zxplane xyplane

      1     0     0
   mode   div   sym

IRONYOKE 1
  1  PACKZ   0.97
 no string  value

EXTRUSION 1
  1      AR1       0   0.1   0.7     12  BHIRON2
 no areaname  zstart  zend  bias  nelem material

PERMANENTMAG2 0

PERMANENTMAG1 0

LAYER 2
  1     4       1      2    1 2 /
  2     4       1      2    3 4 /
 no  symm  typexy  typez blocks

ALGO  /
    1
 algo

DESIGN 0

EULER 0

PEAK 0

TIMETABLE2 0

TIMETABLE1 1
  1    0   10   1 0.001  1  0  0      30      1 /
 no  tds  tde  ff     a  b  c  d  nsteps layers

EDDY  /
    0
 pers

EDDYOPTIONS 0

QUENCHG 0

QUENCHEN 0

QUENCHTM 0

QUENCHP 0

QUENCHS 0

HARMONICTABLE 0

LINEFIELD 0

KVALUES 0

HARMONICOPTION 0

GRAPH 0

GRAPHOPTION 0

PLOT2D 0

PLOT2DOPTION 0

PLOT3D 0

PLOT3DOPTION 0

OBJECTIVE 0

ANSYSOPTIONS /
      1
  scale

      1
  scale

             -90            90            0            0
          ang1         ang2         offx         offy


QUENCH0D /
    0      0     0     0     0      0       0
 qini  tempq  tque  leng  dtdt  deltm  currqm

 
TDEDDY /
      0
   tseddy
